AVP modules reads AVP values for usr_preferences table in SIP-DB.

use is as follows:
   avp_load("caller_uuid");

The parameter is either called_uuid or callee_uuid. It identifies
AVP which stores user's UUID. Then database is dipped with this
UUID.
